OTTAWA VALLEY WASTE RECOVERY CENTRE REQUEST FOR QUOTATION - FIREWOOD

The Ottawa Valley Waste Recovery Centre (OVWRC) is seeking bids for the supply of 40-60 full cords of dry seasoned firewood for Winter 2026/2027. Quotes must be submitted on the vendor quote form and may be received in writing or via e-mail and forwarded to:

Ottawa Valley Waste Recovery Centre
900 Woito Station Rd. RR#4
Pembroke, ON K8A 6W5
c/o Laurie Benjamin, General Manager
lbenjamin@ovwrc.com

RFQ's shall be received until July 30, 2026 @ 1:30 PM at the address given above. RFQ's received by this time, date and at the location specified, shall be opened and read as soon as possible after that time. There will be no public reading.

All wood is to be available from October 2026 until May 2027 on an 'as needed' basis. The successful vendor must be located within 30km of the OVWRC.

The OVWRC intends to transport the sourced firewood using 20 or 40 cubic yard roll-off bins. The bin will be dropped off for loading. The OVWRC will pick up the bins as required. The Centre is looking to procure between 40-60 full cords with 2-4 cord per bin (depending on bin size).

Firewood is to be cut in lengths between 16 and 18 inches. Wood shall be split to a minimum diameter of 6 inches, a maximum diameter of 12 inches and free of any contaminants (dirt, bark and fines). Any combination of wood species is acceptable, however 75% shall be hardwood varieties.

Price per cord shall include any applicable taxes. Bidders are asked to quote on a per cord basis.







OTTAWA VALLEY WASTE RECOVERY CENTRE REQUEST FOR QUOTATION (RFQ) - FIREWOOD

VENDOR QUOTE FORM

VENDOR INFORMATION

Company Name:	 	 Contact Person/Title: 	 Address:		


Phone:
Email:


I, 		,agree to supply 40-60 full cords of dry, seasoned firewood to the Ottawa Valley Waste Recovery Centre for Winter 2026/2027 for the price of $ 	per cord (Including HST).


ACCEPTANCE
All wood will be available from October 2026 until April 2027 on an 'as needed' basis.

Firewood will be cut in lengths between 16 and 18 inches. Wood shall be split to a minimum diameter of 6 inches, a maximum diameter of 12 inches and free of any contaminants (dirt, bark and fines). Any combination of wood species is acceptable, however 75% shall be hardwood varieties.



Submitted By	Date
